**XYZ AIRONE 100 Glass, 6x 120/140mm A-RGB Fan, USB 3.0,Front Glass Design, ATX**  
  
**Immerse yourself in the beauty of transparency and performance with the XYZ AIRONE 100 Glass. This ATX chassis combines an elegant design with exceptional airflow, providing you with an unparalleled gaming experience.**

**Key Features:**

* **Front Glass Design:**The tempered glass front panel of the AIRONE 100 Glass offers a panoramic view of your internal components, turning your PC into an illuminated work of art.
* **Impressive ARGB Lighting:**Enjoy a customizable light show with the 6 included ARGB AIRPULSE 100fans (3 front, 2 top, and 1 rear). Create a unique atmosphere and synchronize the lighting effects with your compatible motherboard.
* **Optimized Airflow:**The AIRONE 100 Glass's design, along with its multiple mounting options for fans and liquid cooling radiators, ensures exceptional ventilation to keep your components cool even under the most demanding workloads.
* **Extensive Compatibility:**This chassis supports ATX, Micro-ATX, and Mini-ITX motherboards, as well as graphics cards up to 320mm and CPU coolers up to 155mm, giving you the flexibility to create the perfect configuration for your needs.
* **Modern Connectivity:**Connect your devices with ease thanks to the USB 3.0 and USB 2.0 ports, as well as the HD audio jacks on the front panel.
* **Easy Maintenance:**Dust filters on the front, top, and bottom ensure your system stays clean and running optimally.

**Technical Specifications:**  
  
**Structure Size:**200 x 440 x 350mm (W x H x D)  
**Case Size:**200 x 445 x 390mm (W x H x D) (with feet)  
**Box Size:**248 x 445 x 490mm (W x H x D)  
**Material:**Steel, Tempered Glass, ABS  
**Side panel:**Left hinged glass  
**Weight:**4/6.2kg  
**Color:**black  
**MB Compatibility:**ATX/M-ATX/ITX  
**Total Possible Fans:**  
3 x 120 / 3x 140mm (Front)  
2 x 120mm (Top)  
1 x 120mm (Rear)  
2 x 120mm (PSU Cover)

**Pre-installed Fans:**  
3 x 140mm (Front) AIRPULSE 100A-RGB (Regular Airflow)  
1 x 120mm (Rear) AIRPULSE 100A-RGB (Regular Airflow)  
2 x 120mm (Top) AIRPULSE 100A-RGB (Regular Airflow)  
**Controller:**No  
**Radiator Mountings:**  
1 x 120/240mm (Front)  
1 x 120mm (Rear)  
**Filter:**Front/Top/Bottom  
**Drive Bays:**2x 3.5/2.5", 2 x 2.5"  
**Power Supply:**Standard ATX  
**Expansion Slots:**7

**I/O Panel:**  
1 x USB3.0  
2x USB2.0  
1 x HD Audio In/Out  
1 x Reset/RGB Switch

**Max GPU Length:**320mm  
**Max CPU Height:** 155mm  
  
**Avaliable colors**   
Black:   
SKU | X-CS-AIRONE1G-B

EAN | 6905290203558  
White:   
SKU | X-CS-AIRONE1G-W  
EAN | 6905290203572