**XYZ AIRWAVE 100**

**Panoramic Elegance, Airflow Performance**

Designed for performance, cooling, and modern aesthetics, the **XYZ AIRWAVE 100** combines a full mesh front panel, tempered glass side panel, and three pre-installed AIRPULSE A-RGB fans. Its clean airflow-focused design and USB Type-C connectivity make it the ideal choice for gamers and creators looking to build an efficient and visually impressive PC.

**Key Features:**

**High-Airflow Mesh Front with A-RGB Illumination**: The full mesh panel ensures superior intake airflow while showcasing vibrant lighting effects from the dual front 140mm AIRPULSE fans.  
**Tempered Glass Side Panel with Sliding Design**: A full-view side panel in tempered glass offers clear visibility of your components and lighting setup, with a smooth sliding mechanism and screwless front for quick access and refined presentation.  
**Triple AIRPULSE 100 A-RGB PWM Fans Included**: Includes two 140mm front fans and one 120mm rear fan, delivering balanced airflow and vivid synchronized lighting with PWM and motherboard sync support (MB SYNC).  
**Advanced Cooling Compatibility**: Supports up to 8 fans and multiple radiator options, including 360mm on the top and 120mm on the rear for high-performance air or liquid cooling configurations.  
**Modern Connectivity with USB Type-C Gen 2**: The front I/O panel includes a Type-C Gen 2 port alongside USB 3.0 and audio ports, offering fast data transfer and versatile connectivity for modern peripherals.  
**Spacious Interior & Hardware Support**: Supports graphics cards up to 420mm (or 380mm with fans installed), CPU coolers up to 165mm, and standard ATX power supplies up to 200mm.

**Technical Specifications:**

**Model**: XYZ AIRWAVE 100  
**Structure Size**: 468 × 215 × 495 mm (L × W × H)  
**Case Size**: 468 × 215 × 495 mm (L × W × H)  
**Box Size**: 550 × 270 × 500 mm (L × W × H)  
**Material**: Steel, Tempered Glass, Mesh  
**Thickness**: SPCC 0.5 mm | 0.6 mm, End Finish  
**Side Panel**: Tempered glass (left side) with sliding design, screwless front  
**Motherboard Support**: ATX / M-ATX / ITX  
**BTF Suppor**t: No  
**Cable Organizer:** Yes, XYZ Velcro  
**Fan Support**:  
2 x 120mm (MBO Bracket)  
3 x 120mm / 2 x 140mm (Top)  
1 x 120mm (Rear)  
3 x 120mm (Bottom)

**Pre-installed Fans**:  
Front MB: 2 x AIRPULSE 100 140mm [REGULAR]  
Rear: 1 x AIRPULSE 100 120mm [REGULAR]  
**Controller**: Included, PWM + ARGB, MB SYNC  
**Radiator Support:**  
Top: 240/280/360mm  
Rear: 120mm  
**Filters**: Top / Bottom  
**Drive Bays:** 1 x 3.5” + 2 x 2.5”  
**Power Supply**: Standard ATX, max 200mm  
**Expansion Slots**: 7  
I/O Panel:  
1 x USB 3.0  
0 x USB 1.1  
1 x Type-C Gen 2  
1 x HD Audio In/Out  
1 x Reset / 1 x LED Control  
**Max GPU Length**: 380mm with fan, 420mm without fan  
**Max CPU Cooler Height**: 165mm

**Avaliable Colors:**

**White**  
SKU | X-CS-AIRWAVE100-W  
EAN | 6978262011567  
**Black**  
SKU | X-CS-AIRWAVE100-B  
EAN | 6978262011574