**XYZ AURORAX 100 PRO – Panoramic Case with Tempered Glass, 5.5” Display, 3 Vortex 120mm A-RGB PWM Fans, XYZ Nexus Software, Type-C**

Take your setup to the next level with the **XYZ AURORAX 100 PRO**, the ultimate panoramic chassis that combines cutting-edge design, advanced cooling, and intelligent system monitoring. Featuring a full tempered glass side panel, an integrated 5.5” LCD display, XYZ Nexus management software, three pre-installed Vortex A-RGB fans, and a USB Type-C port, the **AURORAX 100 PRO** is the perfect choice for creators, enthusiasts, and professional gamers seeking performance, style, and complete control.

**Key Features:**

* **5.5” Modular LCD Display:** View critical system information in real-time, such as CPU and GPU temperatures and loads, or customize the screen with animations, logos, or performance metrics using XYZ Nexus software.   
  In addition, our AURORAX 100 PRO LCD screen is interchangeable, on the side or on the front, the choice of customization is yours.
* **XYZ Nexus Software:** Intuitively manage your system’s performance. Control fans, A-RGB lighting, and configure personalized alerts through a centralized, easy-to-use platform.
* **Elegant Panoramic Tempered Glass Panel:** Showcase your hardware and lighting effects with a full-size tempered glass panel featuring an innovative screw-free sliding system for easy access and a pristine aesthetic.
* **Three Pre-Installed VORTEX 120mm A-RGB PWM Fans:** Achieve optimal cooling with vibrant lighting and silent PWM control, keeping your system cool and visually stunning.
* **Extreme Hardware Compatibility:** Accommodates graphics cards up to 420mm (without fans on the motherboard bracket) or 380mm (with front fans) and CPU coolers up to 165mm tall.
* **High-End Liquid Cooling Ready:** Supports radiators up to 360mm on top and 120mm at the rear, enabling advanced liquid cooling setups.
* **Bottom Mesh Ventilation for Improved Airflow:** A stylish bottom mesh panel maximizes airflow intake to help maintain low temperatures even under heavy load.
* **Premium Finish with Modern Lines:** Built with a high-quality steel frame, fine mesh details, and tempered glass, offering strength, minimalism, and elegance.
* **Next-Generation Connectivity:** Enjoy ultra-fast data transfers with a front panel featuring USB 3.0 and USB Type-C Gen 2 ports.

**Technical Specifications:**

* **Model:** XYZ AURORAX 100 PRO
* **Structure Size:** 468 x 215 x 495 mm (L x W x H)
* **Case Size:** 468 x 215 x 495 mm (L x W x H)
* **Box Size:** 550 x 270 x 500 mm (L x W x H)
* **Material:** Steel, Tempered Glass, Mesh
* **Thickness:** SPCC 0.5 mm / 0.6 mm, end finish
* **Side Panel:** Left side tempered glass with sliding mechanism
* **Display:** Integrated 5.5” LCD
* **Included Software:** XYZ Nexus (monitoring, fan, and lighting control)
* **Motherboard Compatibility:** ATX / M-ATX / ITX
* **BTF Compatibility:** No
* **Cable Management:** XYZ Velcro organizer included
* **Pre-installed Fans:** 3 x Vortex 120mm A-RGB PWM fans
* **Controller:** Included, PWM + ARGB, supports motherboard sync and Nexus control
* **Fan Configuration:**
  + Front (motherboard bracket): 2 x Vortex 120mm A-RGB [reversed]
  + Rear: 1 x Vortex 120mm A-RGB [regular]
* **Additional Fan Support:**
  + 2 x 120mm (motherboard bracket)
  + 3 x 120mm / 2 x 140mm (top)
  + 1 x 120mm (rear)
  + 3 x 120mm (bottom)
* **Radiator Support:**
  + Top: 240/280/360mm
  + Rear: 120mm
* **Filters:** Top / Bottom
* **Drive Bays:** 1 x 3.5” + 2 x 2.5”
* **Power Supply Support:** Standard ATX, up to 200mm
* **Expansion Slots:** 7
* **I/O Panel:**
  + 1 x USB 3.0
  + 1 x USB 1.1
  + 1 x USB Type-C Gen 2
  + 1 x HD Audio In/Out
  + 1 x Reset Button / 1 x LED Control Button
* **Max GPU Length:** 380mm with fans, 420mm without fans
* **Max CPU Cooler Height:** 165mm
* **Cable Management:** Included
* **Packaging:** K=K EPS non-woven fabric bag