**Tempered Glass | Front Mesh | High Airflow | 3x 120mm A-RGB Fans | PWM | Integrated Controller | M-ATX Black**

The **XYZ OMEGA** is a compact and modern chassis designed for those seeking the perfect balance between performance, style, and functionality. With a solid construction combining steel, tempered glass, and mesh, this chassis is optimized for superior airflow and equipped with advanced features like pre-installed A-RGB fans, an integrated controller, and compatibility with high-performance setups.

**Key Features**

* **Tempered Glass with Hinges:** The tempered glass side panel offers a clear view of the interior, adding sophistication and allowing easy access for maintenance.
* **Optimized Front Mesh:** Designed to maximize airflow, ensuring effective cooling even in high-performance configurations.
* **Pre-installed A-RGB Fans:** Equipped with three 120mm A-RGB fans that deliver exceptional cooling performance and customizable lighting effects.
* **Integrated Controller with PWM and A-RGB:** Customize the lighting and adjust fan speeds to maintain a balance between performance and silence.
* **Extensive Compatibility:** Compatible with M-ATX and ITX motherboards, GPUs up to 340mm, and CPU coolers up to 190mm, making it suitable for advanced configurations.
* **Liquid Cooling Ready:** Supports radiators up to 240mm in the front and 120mm in the rear, ideal for liquid cooling setups.

**Technical Specifications**

Structure Dimensions: 230 x 375 x 350 mm (Width x Height x Depth)  
 Total Dimensions: 230 x 390 x 400 mm (Width x Height x Depth)  
 Materials: Steel, tempered glass, mesh, ABS, LED strip  
 Side Panel: Tempered glass with hinges  
 Net Weight: 4.5 kg  
 Gross Weight: 5.3 kg  
 Color: Black  
 Motherboard Compatibility: M-ATX / ITX  
 Cooling Options:  
 - Total possible fans: 2 x 120 mm / 2 x 140 mm (Front), 2 x 120 mm / 2 x 140 mm (Top), 1 x 120 mm (Rear)  
 - Radiators: 1 x 240 mm (Front), 1 x 240 mm (Top), 1 x 120 mm (Rear)  
 Pre-installed Fans:  
 - Model: AIRPULSE 300 120 mm A-RGB PWM  
 - Distribution: Front (2 x 120 mm), Rear (1 x 120 mm)  
 - Specifications: Dimensions: 120 x 120 x 25 mm, Rated Voltage: 12 V (Fan) / 5 V (LED), Speed: PWM 800 - 1500 ± 10% RPM, Airflow: 43.02 CFM, Air Pressure: 1.43 mmH2O, Noise Level: 24.5 dBA, Bearing Type: Hydraulic, Lifetime: > 40,000 hours (at 25 °C)  
 Drive Bays: 2 x 3.5"/2.5", 2 x 2.5"  
 Horizontal PCI-E Slots: 4  
 Vertical PCI-E Slots: 2  
 Power Supply: ATX Standard  
 Dust Filters: Top and Bottom  
 I/O Panel: 2 x USB 3.0, 2 x USB 2.0, 1 x HD Audio In/Out, 1 x Reset/RGB Button  
 Maximum GPU Length: 340 mm  
 Maximum CPU Cooler Height: 190 mm  
 Packaging Dimensions: 280 x 465 x 430 mm (Width x Height x Depth)

**Available Colors**

**White**

• SKU: X-CS-OMEGAM-W

• EAN: 6905290203756

**Black**

• SKU: X-CS-OMEGAM-B

• EAN: 6905290203749