## **XYZ TESSERACT X Panoramic Glass, Dual Chamber, Type C, 7x Pulsar 120mm A-RGB, PWM, MB BTF, ATX**

**Experience a new dimension of gaming with the XYZ Tesseract X. This ATX chassis immerses you in a panoramic visual experience thanks to its tempered glass panels, while offering exceptional performance with its dual-chamber design and superior cooling.**

**Key Features:**

* **Panoramic Design with Tempered Glass:** Enjoy a full view of your components through the tempered glass panels on the front and left side. The Tesseract X transforms your PC into an impressive visual spectacle.
* **Dual Chamber for Impeccable Cable Management:** The dual-chamber design separates the main components from the power supply and cables, keeping the interior of your PC clean and tidy. This improves airflow and facilitates maintenance.
* **Superior Cooling with 7 A-RGB PWM Fans:** Keep your components cool even under the most intense workloads with the seven pre-installed 120mm A-RGB PWM fans. These fans offer powerful airflow and customizable lighting to create a captivating gaming atmosphere.
* **Integrated PWM and ARGB Controller:** Customize and synchronize the lighting and fan speeds with the integrated controller. Create dynamic lighting effects and adjust cooling performance according to your needs.
* **Cableless Motherboard Compatibility (MB BTF):** The Tesseract X is future-ready with support for the latest cableless motherboards with rear connectors, simplifying assembly and reducing cable clutter.
* **Advanced Connectivity with USB Type-C:** Access your high-speed devices with ease thanks to the USB 3.0 and USB Type-C ports on the front panel.

**Technical Specifications:**

* **Structure Size:** 420 x 285 x 380 mm (length x width x height)
* **Case Dimensions:** 420 x 285 x 380 mm (length x width x height)
* **Packaging Dimensions:** 535 x 351 x 440 mm (length x width x height)
* **Material:** Steel, Tempered Glass, ABS
* **Thickness:** 0.6-0.7MM (After paint)
* **Left Side Panel:** Tempered glass with clip
* **Right Side Panel:** Metal with ventilation holes
* **Motherboard Compatibility:** ATX / M-ATX / ITX (Compatible with cableless back plug motherboards)
* **Fan Support:**
  + Motherboard Bracket: 2 x 140/120 mm
  + Top: 2 x 140/3 x 120 mm
  + Rear: 1 x 120 mm
  + Bottom: 3 x 120 mm
* **Pre-installed Fans:**
  + 3 x 120 mm M19 ARGB PWM (side, reverse airflow)
  + 1 x 120 mm M19 ARGB PWM (rear)
  + 3 x 120 mm (bottom, reverse airflow)
* **Controller:** Yes (ARGB and PWM)
* **Liquid Cooling Support:**
  + Motherboard Bracket: 240/280/120 mm
  + Top: 360/280/240 mm
  + Bottom: 360/280/240 mm
* **Dust Filter:** Top/Bottom
* **Drive Bays:** 1 x 3.5" HDD, 2 x 2.5" SSD
* **Power Supply:** Standard ATX (max 240mm)
* **Expansion Slots:** 7
* **I/O Panel:**
  + 2 x USB 3.0
  + 1 x USB Type-C
  + 1 x HD Audio In/Out
  + 1 x Reset/RGB Switch
* **Max GPU Length:** 390mm (MB side with AIO)
* **Packaging Standard:** K=K EPE non-woven fabric bag

**Pre-installed FAN 120 MM Specs (XYZ PULSAR):**

* **Dimensions:** 120 x 120 x 25 mm
* **Bearing Type:** Rifle Bearing
* **Voltage:**
  + Nominal: DC 12V
  + Operation: 10.8 ~ 13.2V
  + Start-up: >5V
* **Current:**
  + Rated: 0.28A ±10% MAX
  + Tag: 0.28A ±10% MAX
  + Blocking: 0.30A ±10% MAX
* **Power Consumption:** 3.36W ±10% MAX
* **Rotation Speed:** 600-1800 ±10% RPM
* **Maximum Air Flow:** 78.64 CFM (ft³/min)
* **Max. Static Pressure:** 1.78mm-H₂O
* **Max. Noise Level:** 36dB(A)
* **Min. Noise Level:** 18.5dB(A)
* **Service Life:** 50,000 hours at 25°C
* **Number of blades:** 9
* **Number of Poles:** 4

Avaliable colors:

Black   
SKU | X-CS-TESSERACTX-B

EAN | 6905290204814  
  
White

SKU | X-CS-TESSERACTX-W  
EAN | 6905290204821