**XYZ TESSERACT X 50 – Panoramic Dual Chamber Case with Tempered Glass, 6x 120mm A-RGB Fans, USB 3.0, ATX Support**

Showcase your build in style with the XYZ TESSERACT X50 — a panoramic dual-chamber case designed to deliver maximum airflow, smart cable management, and stunning visual impact. Featuring 6 pre-installed A-RGB fans, tempered glass side panel without screws, and a reversed GPU cooling layout, it’s the perfect foundation for high-performance gaming and creative systems.

**Key Features:**

1. **Panoramic Tempered Glass Design:** Showcase your components with a full-sized side panel in tempered glass, mounted without screws for a clean and modern look.
2. **Dual Chamber Architecture:** Dedicated space for PSU and cable management at the rear, improving airflow and simplifying building.
3. **6x Pre-installed A-RGB Fans:** Equipped with six AIRPULSE 100 A-RGB 120mm fans, including reversed airflow fans for GPU-side cooling.
4. **High Cooling Capacity:** Supports up to 10 fans and 360mm radiators on top and bottom, ensuring top-tier thermal performance.
5. **USB 3.0 Front Panel & Expandability:** Front I/O includes USB 3.0, HD Audio, and LED control button for lighting customization.
6. **BTF Support:** Future standard thanks to BTF Cableless support for new generation of Motherboards .
7. **ATX Compatibility & Large GPU Support:** Fits full-size ATX motherboards and graphics cards up to 400mm in length.

**Technical Specifications:**

* **Model:** XYZ TESSERACT X 50
* **Structure Size:** 420 x 285 x 390 mm (L x W x H)
* **Case Size:** 420 x 285 x 400 mm (L x W x H)
* **Box Size:** 495 x 360 x 465 mm
* **Material:** Steel, Metal, Airflow Mesh
* **Thickness:** SPCC 0.6 mm / 0.7 mm
* **Color:** Black
* **Side Panel:** Left side tempered glass with clip (no screws), front also screwless
* **Motherboard Support:** ATX / M-ATX / ITX
* **BTF Support:** Yes
* **Pre-installed Fans:** 6 x AIRPULSE 100 A-RGB 120mm
* **Fan Configuration:**
  + Front MB: 3 x 120mm [REVERSED]
  + Bottom: 2 x 120mm [REVERSED, under GPU]
  + Rear: 1 x 120mm [REGULAR]
* **Total Fan Support:**
  + 2 x 140mm or 3 x 120mm (MB bracket)
  + 2 x 140mm or 3 x 120mm (top)
  + 1 x 120mm (rear)
  + 2 x 140mm or 3 x 120mm (bottom)
* **Radiator Support:**
  + 240 / 280 / 360mm (Top)
  + 240 / 280 / 360mm (Bottom)
  + 240 / 280mm (MB bracket)
* **Filters:** Top / Bottom
* **Drive Bays:** 1 x 3.5” + 2 x 2.5”
* **Expansion Slots:** 7
* **Power Supply Support:** Standard ATX, max 200mm
* **Max GPU Length:** 400mm
* **Max CPU Cooler Height:** 175mm
* **I/O Panel:**
  + 1 x USB 3.0
  + 1 x USB 1.1
  + 1 x HD Audio In/Out
  + 1 x Reset / 1 x LED Control
* **Controller:** Not included (Chain Link only)