## **XYZ THERMAX 6 PRO DUO, CPU Air Cooler, 6 Direct Heat pipe, Dual Tower, 2x Vortex 120mm A-RGB fan, with Digital CPU Temp Display**

**Introducing the XYZ Thermax 6 PRO DUO A-RGB. Our ultimate air cooling solution to maintain your processor at peak performance, even during the most intensive tasks. Its dual fan design with customizable ARGB lighting, a digital display showcasing real-time CPU temperatures, 6 heat pipes per side, and its wide socket compatibility make it the ideal choice for gamers and PC enthusiasts seeking both performance and aesthetics.**

**Key Features:**

* **Efficient Cooling:** Maximize heat dissipation with twelve high-quality copper heat pipes (six per tower), ensuring optimal performance at all times.
* **Dual Fan Configuration:** Experience powerful airflow with two high-performance Vortex A-RGB fans operating at 600-2000 RPM, providing 62.7 CFM each with minimal noise of only 18.4dB(A).
* **Real-Time CPU Temperature Monitoring:** Stay informed about your CPU's temperature with the integrated digital display, allowing for proactive adjustments and ensuring optimal performance.
* **Vibrant ARGB Lighting:** Customize and create stunning lighting effects with the integrated ARGB LEDs, adding a touch of style to your PC.
* **Durable Build and Easy Installation:** Enjoy long-lasting and quiet operation thanks to fluid dynamic bearings and a hassle-free installation process.
* **Wide Socket Compatibility:** Versatile cooling for your system with compatibility for a wide range of sockets, including AMD: FM AM3 AM4 AM5 / Intel: LGA 115X/1366/2011/1700/1200/1851
* **Optimized Design:** Maximize airflow and cooling efficiency with the heatsink's optimized design, keeping your CPU running at optimal temperatures even during the most demanding tasks.

**Technical Specifications:**

**Thermax 6 PRO DUO ARGB Heatsink:**

* Socket Compatibility: AMD: FM AM3 AM4 AM5 / Intel: LGA 115X/1366/2011/1700/1200/1851
* Fan Configuration: 2 fans, 0.28A 12VDC, 600-2000 RPM, 62.7 CFM, 33 dB(A) MAX, 18.5dB(A) MIN
* LED Mode: ARGB
* Heatpipes: 6 copper heatpipes per tower (12 total)
* Bearing Type: Fluid dynamic bearing
* Fan Size: 120 mm x 120 mm x 25 mm
* Overall Heatsink Size (Cooler Size): 164 mm x 132 mm x 128 mm
* Additional Feature: Digital CPU Temperature Display

**Vortex A-RGB Fan:**

* Model and Dimensions: Vortex A-RGB, 120x120x25 mm
* Rated Voltage: DC 12V
* Operating Voltage Range: 10.8~13.2V
* Starting Voltage: DC 5V MAX (Rated Voltage, 25℃, 65% RH)
* Rated Current: 0.15A±20%
* Locked Current: 0.20A±20%
* Power Consumption: 1.8W±20%
* Speed: 600-2000±10% RPM (Rated Voltage, 25℃, 65% RH, Free Air)
* Max. Airflow: 62.7 CFM
* Max. Static Pressure: 2.68 mm-H₂O
* Max Noise Level (2000rpm): 32 dB(A)
* Min Noise Level (600rpm): 18.5 dB (A)
* Lifespan: 60,000 hours at 25℃ (MTBF Confidence Level 90%)
* Materials and Construction: PBT RF (frame and blades), Stainless Steel (stator core)
* ARGB Connector: ARGB Head, Female to Male, Daisy Chain

**Available colors:**  
White  
SKU | X-AC-THERPRODUOW6  
  
Black  
SKU | X-AC-THERPRODUOB6