# **XYZ AIRONE 200 GLASS, 5x A-RGB 120/140mm Fan, USB 3.0,Front Tempered Glass Design, ATX**

**Immerse yourself in an unparalleled ventilation and performance experience with the XYZ AIRONE 200 Glass edition. This ATX chassis combines a tempered glass front panel design with exceptional airflow on the sides, giving you the freedom to build a powerful system and keep it cool even under the most demanding workloads.**

**Key Features:**

* **Tempered glass Design for Maximum style:** The AIRONE 200 Glass, impresses with a tempered glass front finish and side air intakes for unique airflow efficiency and performance.
* **Impressive ARGB Lighting with MB Sync:** Enjoy a customizable light show with the 5 included ARGB AIRPULSE 100 fans (2 front, 2 top, and 1 rear). Create a unique atmosphere and synchronize the lighting effects with your compatible motherboard thanks to the MB LIGHT SYNC feature.
* **Extensive Compatibility:** This chassis supports ATX, Micro-ATX, and Mini-ITX motherboards, as well as graphics cards up to 320mm and CPU coolers up to 155mm, giving you the flexibility to create the perfect configuration for your needs.
* **Extreme Liquid and Air Cooling:** Keep your system cool under any workload with extensive support for liquid and air cooling. The AIRONE can accommodate radiators up to 240mm on the front and 120mmon the rear, as well as offering space for up to 7 fans.
* **Tempered Glass Side Panel:** Admire your internal components through the elegant tempered glass side panel. The AIRONE 200 Glass becomes a showcase for your high-end hardware.
* **Modern Connectivity and Cable Management:** Connect your devices with ease thanks to the USB 3.0 and USB 2.0 ports, as well as the HD audio jacks on the front panel. Additionally, the Fans Chain feature allows you to daisy-chain the fans for cleaner and more efficient cable management.

**Technical Specifications:**

* **Structure Size:** 200 x 440 x 350 mm (W x H x D)
* **Case Size:** 200 x 445 x 390 mm (W x H x D) (with feet)
* **Packaging Dimensions:** 248 x 445 x 490 mm (W x H x D)
* **Material:** Steel, Tempered Glass, Glass, ABS
* **Side panel:** Left hinged glass
* **Weight:** 4.55 kg / 5.33 kg
* **Color:** black
* **MB Compatibility:** ATX/M-ATX/ITX
* **Total Possible Fans:**
  + 3 x 120 / 2x 140mm (Front)
  + 2 x 120mm (Top)
  + 1 x 120mm (Rear)
  + 2 x 120mm (PSU Cover)
* **Pre-installed Fans:**
  + 2 x 140mm (Front) AIRPULSE 100 ARGB
  + 1 x 120mm (Rear) AIRPULSE 100 ARGB
  + 2 x 120mm (Top) AIRPULSE 100 ARGB
* **Controller:** No
* **MB LIGHT SYNC:** Yes
* **Fans Chain:** Yes
* **Radiator Mountings:**
  + 1 x 280/240mm (Front)
  + 1 x 120mm (Rear)
* **Filter:** Top/Bottom
* **Drive Bays:** 2x 3.5/2.5", 2 x 2.5"
* **Power Supply:** Standard ATX
* **Expansion Slots:** 7
* **I/O Panel:**
  + 1 x USB3.0
  + 2x USB2.0
  + 1 x HD Audio In/Out
  + 1 x Reset/RGB Switch
* **Max GPU Length:** 320mm
* **Max CPU Height:** 155mm

**Avaliable colors**  
Black  
SKU | X-CS-AIRONE2G-B / EAN | 6905290203602

Black / White   
SKU | X-CS-AIRONE2G-BW

White  
SKU | X-CS-AIRONE2G-W