**XYZ AIRONE 300 Glass, 6x 120mm A-RGB Fan,ARGB Controller, USB 3.0,Front Glass Design, ATX**  
  
**Immerse yourself in crystalline elegance and exceptional performance with the XYZ AIRONE 300 Glass. This ATX chassis combines a panoramic front glass design with stunning ARGB lighting, creating a captivating gaming atmosphere. Enjoy efficient cooling and impeccable cable management in a compact and functional chassis.**

**Key Features:**

* **Front Glass Design:** The tempered glass front panel of the AIRONE 300 Glass offers a panoramic view of your internal components and the ARGB lighting of the fans, turning your PC into a luminous work of art.
* **6 Included A-RGB Fans:** Enjoy a customizable light show with the 6 included AIRPULSE 100 A-RGB fans (3 front, 2 top, and 1 rear). Create a unique ambiance and synchronize the lighting effects with the integrated ARGB controller.
* **Integrated ARGB Controller:** Easily customize and control the fan lighting with the included ARGB controller. Create dynamic effects and choose from a wide range of colors to tailor the aesthetic to your style.
* **Efficient Cooling:** Keep your components cool with optimized airflow thanks to the multiple mounting options for fans and liquid cooling radiators. The AIRONE 300 Glass supports radiators up to 280/240mm in the front, 240mm on the top, and 120mm in the rear.
* **Wide Compatibility:** This compact chassis supports ATX, Micro-ATX, and Mini-ITX motherboards, as well as graphics cards up to 335mm (or 310mm if using an AIO) and CPU coolers up to 160mm.
* **USB 3.0 Connectivity:** Connect your high-speed devices with ease thanks to the USB 3.0 port on the front panel, along with two USB 2.0 ports and HD audio jacks.  
  **Technical Specifications:**  
  **Case Dimensions**
* **Structure sizes:** 190 x 440 x 400 mm (W x H x D)
* **Case Size:** 190 x 445 x 400 mm (W x H x D)
* **Packaging Size:** 242 x 481 x 437 mm (W x H x D)

**Material**

* Steel, Tempered Glass, ABS, LED strip

**Side panel**

* Left side metal with 4 screws tempered glass

**Weight**

* 5.5/4.4 kg

**MB Compatibility**

* ATX/M-ATX/Mini-ITX

**Total Possible Fans**

* 3 x 120 mm (Front)
* 2 x 120 mm (Top)
* 1 x 120 mm (Rear)
* 2 x 120 mm (PSU Cover)

**Pre-installed Fans**

* 3 x 120 mm AIRPULSE 100 ARGB (Front)
* 1 x 120 mm AIRPULSE 100 ARGB (Rear)
* 2 x 120 mm AIRPULSE 100 ARGB (Top)

**Controller**

* Yes (ARGB with on/off function)

**Radiator Mountings:**

* 1 x 120/240mm (Front)
* 1 x 120mm (Rear)

**Filter**

* Top panel with dust filter

**Drive Bays**

* 2x 3.5/2.5", 2 x 2.5"

**Power Supply**

* Standard ATX

**Expansion Slots**

* 7

**I/O Panel:**

* 1 x USB3.0
* 2x USB2.0
* 1 x HD Audio In/Out
* 1 x Reset/RGB Switch

**Max GPU Length:**

* 335 mm (310mm if using AIO)

**Max CPU Height:**

* 160mm

**Available colors**

* **Black:** SKU X-CS-AIRONE3G-3B
* **White:** SKU X-CS-AIRONE3G-3W