**XYZ AIRONE 300 X Mesh, 6x 120mm A-RGB Fan, USB C GEN2, Mesh Front Design ATX**

**Introducing the XYZ AIRONE 300 X Mesh, the next generation of our popular AIRONE 300 chassis.** Designed to exceed the expectations of even the most demanding gamers and PC enthusiasts, the AIRONE 300 X Mesh offers unmatched airflow, a modern design, and a host of improvements that make it the perfect choice for building your dream PC.

**Key Features:**

* **Unmatched Cooling:** Equipped with 6 pre-installed 120mm ARGB fans, the AIRONE 300 X Mesh ensures your system stays cool and stable, even during the most intense gaming sessions.
* **Stunning Design:** The tempered glass side panel allows you to proudly showcase your PC components, while the mesh front panel ensures excellent airflow.
* **Limitless Expandability:** With support for multiple radiators and a wide range of components, the AIRONE 300 X Mesh gives you the flexibility to build the PC of your dreams.
* **Complete Connectivity:** The front I/O panel includes a USB 3.0 port, a USB Type-C Gen2 port, and HD audio connectors for easy connection of your peripherals.
* **Customizable Lighting:** The pre-installed ARGB fans allow you to personalize your chassis lighting to match your style.

**Technical Specifications**

* **Dimensions:** 216 x 445 x 365 mm (Width x Height x Depth)
* **Material:** Steel, Tempered Glass, ABS
* **Side Panel:** Sliding Tempered Glass
* **Motherboard Compatibility:** ATX/Micro-ATX/ITX
* **Pre-installed Fans:** 6x 120mm ARGB (AIRPULSE 100)
  + 3x 120mm front
  + 2x 120mm top
  + 1x 120mm rear
* **Fan Specifications:** Dimensions: 120x120x25mm; Rated Voltage: DC 12V; Rated Current: 141mA; Speed: 1100RPM; Airflow: 32.5 CFM; Noise: 25.3 dBA
* **Radiator Compatibility:** Top: 1x 240/280mm; Rear: 1x 120mm
* **Storage:** 2x 3.5"/2.5", 2x 2.5"
* **Power Supply:** Standard ATX
* **PCI-E Slots:** 7 horizontal, 0 vertical
* **Front I/O Panel:** 1x USB 3.0, 1x USB Type-C Gen2, 1x HD Audio, 1x Reset/RGB Switch button
* **Maximum GPU Length:** 330mm/305mm (with fan)
* **Maximum CPU Cooler Height:** 175mm
* **Package Dimensions:** 270 x 430 x 505mm (Width x Height x Depth)
* **Available Colors:**
  + SKU | X-CS-AIRONE3XM-B
  + SKU | X-CS-AIRONE3XM-W