**XYZ AIRONE 50 Mesh, 4x 120/140mm A-RGB Fan, USB 3.0,Front Mesh Design, ATX**

**Immerse yourself in an unparalleled ventilation and performance experience with the XYZ AIRONE 50 Mesh. This ATX chassis combines a mesh front panel design with exceptional airflow, giving you the freedom to build a powerful system and keep it cool even under the most demanding workloads.**

**Key Features:**

* **Mesh Design for Maximum Ventilation:** The AIRONE 50 Mesh's high-quality mesh front panel allows for massive airflow, ensuring optimal cooling for your high-performance components. Say goodbye to overheating and enjoy intense gaming sessions without worry.
* **Impressive ARGB Lighting:** Enjoy a customizable light show with the 4 included ARGB AIRPULSE 50 fans (3 front, and 1 rear). Create a unique atmosphere and synchronize the lighting effects with your compatible motherboard.
* **Extensive Compatibility:** This chassis supports ATX, Micro-ATX, and Mini-ITX motherboards, as well as graphics cards up to 320mm and CPU coolers up to 155mm, giving you the flexibility to create the perfect configuration for your needs.
* **Extreme Liquid and Air Cooling:** Keep your system cool under any workload with extensive support for liquid and air cooling. The Airwave can accommodate radiators up to 240mm on the front and 120 on rear as well as offering space for up to 8 fans.
* **Tempered Glass Side Panel:** Admire your internal components through the elegant tempered glass side panel. The AIRONE 100 Mesh becomes a showcase for your high-end hardware.
* **Modern Connectivity:** Connect your devices with ease thanks to the USB 3.0 and USB 2.0 ports, as well as the HD audio jacks on the front panel.

**Technical Specifications:**

* **Structure Size:** 200 x 440 x 350mm (W x H x D)
* **Case Size:** 200 x 445 x 390mm (W x H x D) (with feet)
* **Box Size:** 248 x 445 x 490mm (W x H x D)
* **Material:** Steel, Tempered Glass, Mesh, ABS
* **Side panel:** Left hinged glass
* **Weight:** 4.92/5.73kg
* **MB Compatibility:** ATX/M-ATX/ITX
* **Total Possible Fans:**
  + 3 x 120 / 3x 140mm (Front)
  + 2 x 120mm (Top)
  + 1 x 120mm (Rear)
  + 2 x 120mm (PSU Cover)
* **Pre-installed Fans:**
  + 3 x 140mm (Front) AIRPULSE 100 ARGB
  + 1 x 120mm (Rear) AIRPULSE 100 ARGB
* **Controller:** No
* **Radiator Mountings:**
  + 1 x 120/240mm (Front)
  + 1 x 120mm (Rear)
* **Filter:** Top/Bottom
* **Drive Bays:** 2x 3.5/2.5", 2 x 2.5"
* **Power Supply:** Standard ATX
* **Expansion Slots:** 7
* **I/O Panel:**
  + 1 x USB3.0
  + 2x USB2.0
  + 1 x HD Audio In/Out
  + 1 x Reset/RGB Switch
* **Max GPU Length:** 320mm
* **Max CPU Height:** 155mm

**Available Colors：**

**Black**

SKU: X-CS-AIRONE50-M-B

EAN: 6978262011352