**XYZ NEUTRON ATX Panoramic Tempered Glass Chassis, Dual Chamber, 4x 120mm A-RGB, PWM, Built-in Controller**  
  
**Elevate your gaming setup to the next level with the XYZ NEUTRON. This ATX chassis offers you a panoramic view of your components thanks to its two tempered glass panels, while its dual-chamber design ensures impeccable cable management and optimized airflow.**

**Key Features:**

* **Panoramic Design with Dual Tempered Glass:** Immerse yourself in the beauty of your build through the two tempered glass panels: front and side. Enjoy an unobstructed view of your components and create an impressive centerpiece for your gaming setup.
* **Dual Chamber & outstanding compatibility:** The NEUTRON's dual-chamber design separates the main components from the power supply and cables, allowing for clean and tidy cable management. Hide unsightly cables and improve airflow for optimal performance. NEUTRON´s has the capacity to accommodate up to 360mm liquid coolers, up to 400mm graphics cards, 160mm CPU Air Coolers and up to 10 fans for unique airflow.
* **Advanced Cooling with 4 AURAX A-RGB PWM Fans:** Keep your components cool even during the most intense gaming sessions thanks to the four included 120mm AURAX A-RGB PWM fans. These fans offer powerful airflow and customizable lighting to create a captivating gaming atmosphere.
* **Integrated Controller with PWM & MB Sync:** Customize and synchronize the lighting of the AURAX fans and other compatible ARGB components with the integrated controller. Create dynamic and harmonious lighting effects that match your style.
* **LCD Screen for Screen Duplication:** Take customization to the next level with the integrated LCD screen on the front panel. Duplicate your PC screen or display important system information, such as temperature and resource usage, for total control over your gaming experience.

**Technical Specifications:**

* **Structure Dimensions:** 418 x 280 x 410 mm (length x width x height)
* **Case Dimensions:** 418 x 280 x 435 mm (length x width x height) (with feet)
* **Packaging Dimensions:** 492 x 343 x 495 mm (length x width x height)
* **Material:** Steel, Tempered Glass, ABS
* **Left Side Panel:** Tempered glass with clip
* **Right Side Panel:** Metal
* **Weight:** 8.54 kg / 7.28 kg
* **I/O:** 2 x USB 3.0 + 1 x USB 2.0 + HD Audio, power button + reset button + LCD screen
* **PSU Position & Type:** Bottom, ATX
* **Motherboard Support:** ATX / Micro-ATX / Mini-ITX
* **Drive Bays:**
  + 2 x 3.5" HDD
  + 2 x 2.5" SSD
* **Fan Support:**
  + Bottom: 3 x 120 mm
  + Motherboard Bracket: 3 x 120 mm
  + Top: 3 x 120 mm
  + Rear: 1 x 120 mm
* **Pre-installed Fans:**
  + 3 x 120 mm AURAX ARGB PWM (motherboard bracket, reverse airflow)
  + 1 x 120 mm AURAX ARGB PWM (rear)
* **Controller:** Yes (ARGB and PWM, with MB Sync)
* **Liquid Cooling Support:**
  + Top: 360/280/240 mm
  + Rear: 120 mm
* **Dust Filter:** Top and bottom
* **PCI Expansion Slots:** 7
* **Maximum Graphics Card Length:** 400 mm
* **Maximum CPU Cooler Height:** 160 mm
* **Packaging Standard:** K=K + EPS and brown cardboard box
* Outline Dimension: 64.3 x 231.3 (typ)
* Inches: 8.8"
* Display Area: 54.72(H) x 218.88(V)
* Number of Pixels: 1920x480
* Pixel Pitch: 0.114(H) x 0.114(V)
* Pixel Arrangement: RGB Vertical Stripe
* Display Mode: Normally Black
* NTSC: 50 (typ.)
* Surface Treatment: HC
* Weight: (110)g (typ.)
* Power Consumption:
* Logic: 0.65 (Max)
* Refresh Rate 60Hz
* BL System: 2.8 (Max) @ Black pattern w/o LED driver

**Available Colors:**

**White**

SKU: X-CS-NEUTRON-W

EAN: 6978262010348

**Black**

SKU: X-CS-NEUTRON-B

EAN: 6978262010331