**XYZ TESSERACT ARGB, 3D Panoramic Glass,Dual Chamber, Type C,4x Vortex 120mm A-RGB,PWM,MB BTF, ATX**

**Defy the limits of space and time with the XYZ Tesseract, an engineering masterpiece that fuses three-dimensional design with cutting-edge gaming performance and awesome A-RGB Design for your custom gaming experience.**

**Key Features:**

* **4D Tesseract Design:** Inspired by the four-dimensional hypercube, the Tesseract redefines the aesthetic of gaming cases. Its angular lines and tempered glass panels create a captivating visual effect that will transport you to another dimension.
* **Extreme Cooling with Vortex A-RGB:** **:** Keep your components cool and running at peak performance with the 4 Vortex A-RGB fans (3 front reversed (Vortex PRO) , and 1 rear regular). The optimized airflow, customizable A-RGB lighting, and **wireless daisy-chainable design** of the Vortex fans create a symphony of color and efficiency.
* **Wide Compatibility and Flexibility:** The Tesseract supports ATX, M-ATX, and ITX motherboards, graphics cards up to 400mm, and CPU coolers up to 165mm. It offers space for multiple storage and liquid cooling configurations, giving you the freedom to customize your system to your liking.
* **Panoramic Viewing Experience:** Showcase your high-end components in all their glory with the Tesseract's triple tempered glass panels on the front, side, and top. Enjoy an unobstructed view of your hardware and create a stunning centerpiece for your gaming setup.
* **Back free routed MB compatible: Tesseract is designed to be compatible with the latest motherboards without front cables, simplifying the mounting process and reducing cable clutter.**
* **USB Type-C Gen 2 Connectivity:** Access your high-speed devices with ease thanks to the located USB Type-C port on the top I/O panel.

**Technical Specifications:**

* **I/O:** 2 x USB 3.0 + USB Type-C GEN 2 (top) + HD Audio
* **Left Side Panel:** Tempered glass with clip
* **Right Side Panel:** Metal with ventilation holes
* **Material:** SPCC 0.7 mm | 0.8 mm , End Finish
* **PSU Position & Type:** Bottom, ATX
* **Motherboard Support:** ATX / M-ATX / ITX (with rear plug support)
* **Fan Support:**
  + 3 x 120mm on motherboard bracket
  + 1 x 120mm rear
  + 3 x 120mm bottom
* **Fans Included:** 4 x XYZ VORTEX A-RGB (3 reverse airflow (PRO), 1 regular airflow)
* **Integrated ARGB Controller:** YES
* **Water Cooling Support:**
  + 360/280/240mm on motherboard bracket
  + 360/280/240mm bottom
  + 120mm rear
* **Drive Bays:**
  + 1 x 3.5" HDD
  + 2 x 2.5" SSD
* **PCI Expansion Slots:** 9
* **Max GPU Length:** 400mm
* **Max CPU Cooler Height:** 165mm
* **Magnetic Dust Filter:** Bottom
* **Dimensions:** 424 x 285 x 455mm
* **Bearing:** FDB
* **Voltage:** 12V (rated), 10.8-13.2V (operating), 5V (startup)
* **Current:** 0.20A (rated), 0.21A (stall)
* **Power Consumption:** 1.80W
* **Speed:** 600-2000 RPM
* **Airflow:** 62.7 CFM
* **Static Pressure:** 2.68 mm-H₂O
* **Noise:** 18.5-32.0 dB(A)
* **Lifespan:** 60,000hrs (25°C)
* **Blades:** 9
* **Poles:** 4

**Avaliable colors：**

**White**

• SKU: X-CS-TESSERACT-W

• EAN: 6978262010904

**Black**

•SKU: X-CS-TESSERACT-B

• EAN: 6978262010898