**XYZ TESSERACT DIGITAL - Tempered Glass, Mesh, Digital Temperature Display, 4x Pulsar 120mm A-RGB PWM, Type-C, ATX**

Experience the next level in performance and aesthetics with the XYZ TESSERACT DIGITAL. Designed for enthusiasts seeking a perfect balance between airflow, functionality, and style, this dual-chamber ATX case offers a premium building experience and exceptional performance.

**Key Features:**

* **Dual Chamber Design:** Maximizes airflow and cable management by separating the power supply and hard drives from the rest of the components for better thermal management.
* **Total Airflow with Full Mesh Front Panel:** The full mesh front panel ensures optimal airflow, keeping your components cool even during the most intense gaming sessions.
* **Panoramic Design with Tempered Glass:** The tool-free tempered glass side panel provides a panoramic view of your setup, allowing you to showcase your high-end components.
* **Digital Temperature Display:** Monitor your system temperature in real-time with the integrated digital display on the front panel, keeping you informed about your PC's performance.
* **4x Pulsar 120mm A-RGB PWM Fans Included:** Enjoy superior cooling and vibrant lighting with the 4 pre-installed Pulsar A-RGB PWM fans, synchronizable with your motherboard for custom lighting effects.
* **USB Type-C Gen 2 Port:** Connect your latest generation devices with the high-speed USB Type-C Gen 2 port on the front panel for fast and efficient data transfer.
* **ATX Compatibility:** Supports ATX, Micro-ATX, and ITX motherboards, offering flexibility to build your dream system.

**Technical Specifications:**

* **Dimensions:** Structure: 443 x 280 x 415 mm (L x W x H), Case: 443 x 280 x 440 mm (L x W x H), Packaging: 505 x 345 x 518 mm (L x W x H)
* **Material:** SPCC Steel (0.5 mm / 0.6 mm), Tempered Glass, Mesh
* **Motherboard Compatibility:** ATX, Micro-ATX, ITX
* **Pre-installed Fans:** 3 x 120 mm (Front), 1 x 120 mm (Rear) - Pulsar A-RGB PWM
* **Total Fan Support:** 3 x 120 mm (Top), 3 x 120 mm (MB Tray), 3 x 120 mm (Bottom), 3 x 120 mm (Front), 1 x 120 mm (Rear)
* **Radiator Support:** 240/280/360 mm (Top), 240/280/360 mm (MB Tray), 120 mm (Rear)
* **Drive Bays:** 3 x 3.5", 2 x 2.5"
* **Expansion Slots:** 7
* **Maximum GPU Length:** 420 mm
* **Maximum CPU Height:** 175 mm
* **Maximum Power Supply Size:** 140/160/200 mm
* **I/O Ports:** 2 x USB 3.0, 1 x USB Type-C Gen 2, 1 x HD Audio In/Out, 1 x Reset/LED
* **Dust Filter:** Bottom
* **Cable Management:** Yes
* **ARGB/PWM Controller:** Included, motherboard synchronization (MBSYNC)

**Available Colors:**

* White: X-CS-TESS-DIG-W
* Black: X-CS-TESS-DIG-B