## **TITANIUM MESH Elegance Style, Airflow Performance**

**The **XYZ TITANIUM MESH** is an ATX mid-tower chassis designed for gamers and enthusiasts seeking a perfect balance between aesthetics and functionality. With a front mesh design optimized for superior airflow, four pre-installed 120mm A-RGB PWM fans, and an integrated controller, this chassis ensures your system stays cool and looks spectacular even during the most intense gaming sessions.**

**Key Features:**

****Front Mesh Design for Optimal Airflow:****  
The high-quality front mesh allows for unrestricted air intake, providing exceptional cooling for all your components. This is crucial for maintaining peak performance during long gaming sessions or demanding tasks.  
****4 Pre-installed 120mm A-RGB PWM Fans:****  
Equipped with four AIRPULSE 300 120mm fans, this chassis offers powerful and quiet cooling right out of the box. Customizable A-RGB lighting allows you to create stunning visual effects that synchronize with the rest of your setup.  
****Integrated PWM + A-RGB Controller with MBSYNC:****  
The integrated controller allows you to easily manage fan speeds and A-RGB lighting effects. Additionally, MBSYNC (Motherboard Sync) compatibility lets you synchronize lighting with your motherboard for a unified light show.  
****Tempered Glass Side Panel****:  
The clip-on tempered glass side panel allows you to showcase the interior of your system, highlighting your components and A-RGB lighting. The tool-free design facilitates easy access and installation.  
****Extensive Compatibility and Expansion****:  
Supports ATX, MATX, and Mini-ITX motherboards, and offers multiple storage options with bays for 3.5″ and 2.5″ drives. With 7 horizontal and 2 vertical PCI-E slots, you have the flexibility to install multiple graphics cards and other expansion devices. Also supports 120mm radiators at the rear, 240mm radiators on the motherboard tray, and 360mm radiators at the top, providing ample options for liquid cooling solutions.  
****Modern Connectivity:****  
o The front I/O panel includes 2 USB 3.0 ports, 2 USB 2.0 ports, HD audio connectors, and a button to control RGB lighting, providing easy and quick access to your devices and peripherals.

**Technical Specifications:**

****Dimensions****: 210 x 480 x 454 mm (Width x Height x Depth)  
****Material****: Steel, Tempered Glass, Mesh, ABS  
****Net Weight****: 6.5 kg  
****Gross Weight****: 7.64 kg  
****Color****: Black  
****Motherboard Compatibility****: ATX, MATX, Mini-ITX  
****Pre-installed Fans****: 4 x 120mm A-RGB PWM (3 front, 1 rear)  
****Expansion Slots****: 7 horizontal, 2 vertical  
****Drive Bays****: 2 x 3.5″/2.5″, 2 x 2.5″  
****Maximum GPU Length****: 400 mm  
****Maximum CPU Height****: 168 mm  
****Power Supply****: Standard ATX  
****I/O Panel****:  
2 x USB 3.0  
2 x USB 2.0  
HD Audio  
RGB/Reset Button  
****Radiator Compatibility****:  
1 x 240 mm (motherboard tray)  
1 x 360 mm (top)  
1 x 120 mm (rear)

Controller: Yes (ARGB and PWM)

Dust Filter: Top/Bottom

Power Supply: Standard ATX (max 240mm)

****Available Colors：****  
****Black****  
SKU | X-CS-TITANIUMMESH-B  
EAN | 6978262010317