**XYZ TITANIUM VIEW Tempered Glass, 4x 120mm A-RGB Fan, PWM,Integrated Controller, Panoramic 2D Design,Type C,USB 3.0, ATX**  
  
**Elevate your gaming experience with the XYZ TITANIUM VIEW. This ATX chassis offers a panoramic view of your components through its dual tempered glass panels, while ensuring optimal airflow and cable management for peak performance.**

**Key Features:**

1. **Panoramic 2D Design with Tempered Glass:** Immerse yourself in the beauty of your build through the dual tempered glass panels on the front and left side. Showcase your high-end hardware and create a stunning centerpiece for your gaming setup.
2. **Efficient Cooling with 4 A-RGB Fans:** Keep your components cool and running at their best with the four pre-installed 120mm A-RGB fans (3 front-mounted with reverse airflow and 1 rear regular airflow). These fans provide powerful airflow and customizable lighting to create a captivating gaming atmosphere.
3. **Integrated PWM & ARGB Controller:** Take control of your system's aesthetics and performance with the integrated controller. Customize fan speeds and ARGB lighting effects, and synchronize them with your motherboard for a seamless and immersive experience.
4. **Extensive Cooling Support:** The TITANIUM VIEW accommodates a variety of cooling solutions, with support for up to 7 fans and radiators up to 360mm on top, 240mm on the motherboard tray, and 120mm at the rear.
5. **Ample Space and Compatibility:** This chassis supports ATX, Micro-ATX, and Mini-ITX motherboards, as well as graphics cards up to 400mm and CPU coolers up to 168mm. It also features convenient front panel connectivity with 2 USB 3.0 ports, 2 USB 2.0 ports, and a USB Type-C port.

**Technical Specifications:**

* **Structure Size:** 210 x 465 x 420mm (W x H x D)
* **Case Dimensions:** 210 x 480 x 446mm (W x H x D)
* **Box Size:** 270 x 525 x 525mm (W x H x D)
* **Material:** Steel, Tempered Glass, ABS
* **Side Panel:** Left side clip-on tempered glass
* **Weight:** 7.52/8.82 kg
* **Color:** Black
* **MB Compatibility:** ATX / MATX / Mini-ITX
* **Total Possible Fans:**
  + 3 x 120mm (Motherboard Bracket)
  + 3 x 120mm (Top)
  + 1 x 120mm (Rear)
  + 2 x 120mm (Power Cover)
* **Pre-installed Fans:**
  + 3 x 120mm (Front) AURAX 120MM ARGB PWM (REVERSE)
  + 1 x 120mm (Rear) AURAX 120MM ARGB PWM
* **Controller:** YES, PWM+ARGB
* **Radiator Mountings:**
  + 1 x 240mm (Motherboard Tray)
  + 1 x 360mm (Top)
  + 1 x 120mm (Rear)
* **Filter:** Top/Bottom
* **Drive Bays:** 2x 3.5/2.5", 2 x 2.5"
* **Power Supply:** Standard ATX
* **Expansion Slots:** 7+2
* **I/O Panel:**
  + 2 x USB3.0
  + 2 x USB2.0
  + 1 x Type-C
  + 1 x HD Audio In/Out
  + 1 x Reset/RGB Switch
* **Max GPU Length:** 400mm
* **Max CPU Height:** 168mm

**Pre-installed FAN 120 MM Specs (AURAX 120MM):**

* **Dimensions**: 120 x 120 x 25 mm
* **Speed:** 1600-1800 RPM ± 10%
* **Airflow:** 53.71 CFM
* **Air Pressure:** 1.28 mmH2O
* **Noise Level:** 33.5 dBA
* **Bearing Type:** Hydraulic
* **Power Consumption:**

Fan: 2.4W (12V)

LED: 4W (5V)

**Voltage:**

Rated: 12V DC

Operation: 5-13.2V DC

Start-up: >5V

**MTTF: >40000 hours (at 25°C)**

**Avaliable colors:**

**Black**

SKU: X-CS-TITANIUM300-B

EAN: 6978262010324