# **XYZ TRIFECTA 3D Panoramic Glass, Type C GEN 2, PCI-E Reversible, 2x Vortex 120mm A-RGB, PWM, MB BTF BACK ROUTE , ATX**

**Expand your vision and take your gaming setup to the next level with the XYZ Trifecta, the panoramic case that combines cutting-edge aesthetics with intelligent functionality.**

**Key Features:**

1. **Trifecta Panoramic Design:** Immerse yourself in a captivating visual experience thanks to the Trifecta's three tempered glass panels, covering the front, side, and top. View your high-end hardware from every angle and turn your desk into a technological showcase.
2. **Superior Cooling with Vortex A-RGB:** Keep your components cool and running at peak performance with the 2 included Vortex A-RGB fans. The optimized airflow, customizable A-RGB lighting and the performance of the Vortex fans create a symphony of color and efficiency.
3. **Customizable Versatility:** The Trifecta adapts to your needs with reversible PCI-E slots, allowing you to install your graphics card vertically or horizontally without the need for additional accessories. Its spacious design also supports ATX, Micro-ATX, and Mini-ITX motherboards, giving you the freedom to create the perfect configuration.
4. **Impeccable Cable Management:** Keep the inside of your case tidy and optimized with the 24mm of cable management space and included rubber accessories. Say goodbye to tangled cables and improve airflow for optimal performance.
5. **Future-Ready:** The Trifecta offers compatibility with liquid cooling up to 360mm on the motherboard tray and 120mm on the rear, ensuring your system stays cool even during the most intense gaming sessions. It's also designed to be compatible with the latest cableless motherboards, keeping you at the forefront of technology.
6. **Advanced Connectivity:** Access your high-speed devices with ease thanks to the high-speed USB 3.0 ports and the conveniently located USB Type-C Gen 2 port on the top I/O panel.

**Technical Specifications:**

* **Left Panel:** 3 x Tempered Glass
* **Right Panel:** Metal
* **Material:** SPCC 0.6mm | 0.7mm, End-Finish
* **PSU:** Bottom, ATX (150-180mm)
* **Motherboard:** ATX / Micro-ATX / Mini-ITX
* **Bays:** 1 x 3.5" HDD + 1 x 2.5" SSD or 2 x 2.5" SSD
* **Fans:**
* Support: 3x120mm (motherboard), 1x120mm (rear), 3x120mm (PSU shroud)
* Included: 2x Vortex PWM A-RGB
* 1 Regular Airflow (rear) / 1 Reversed Airflow (Bottom)
* **Integrated Controller**: Yes
* **Functions**: A-RGB+PWM+MBYSNC
* **BTF Motherboard Back route**: Yes
* **Liquid Cooling:** 360mm (motherboard), 120mm (rear)
* **PCI Slots:** 7+2
* **Max GPU Length:** 400mm
* **Max CPU Cooler Height:** 180mm
* **Cable Management:** 24mm
* **I/O:** 1 x USB 3.0
* 1 x USB Type-C Gen 2
* HD Audio
* **Dust Filter:** Magnetic, bottom
* **Dimensions:** 440x232x480mm
* **Packaging Size:** 270x525x525mm

**Vortex A-RGB Fan Specifications:**

* **Bearing:** FDB (Fluid Dynamic Bearing)
* **Rated Voltage:** DC 12V
* **Operating Voltage:** 10.8 ~ 13.2V
* **Starting Voltage:** DC 5 V MAX
* **Rated Current:** 0.20A ± 20% MAX (Labeled Current: 0.20A)
* **Locked Current:** 0.21A ± 20% MAX
* **Power Consumption:** 1.80W ± 20% MAX
* **Speed:** 600-2000 ± 20% RPM
* **Max. Airflow:** 62.7 CFM (ft³/min)
* **Max. Static Pressure:** 2.68 mm-H₂O
* **Max Noise Level:** 32.0 dB(A)
* **Min. Noise Level:** 18.5 dB(A)
* **Life:** 60,000hrs at 25°C
* **No. of Blades:** 9 Blades
* **No. of Poles:** 4 Poles