## **XYZ THERMAX 6 PULSAR CPU Air Cooler, Digital Temperature Display, 6 Direct Heat Pipes, Pulsar 120mm A-RGB Fan, Black**

**Master the heat with style and precision**

The XYZ THERMAX 6 PULSAR A-RGB is our CPU air cooler that combines exceptional performance with an eye-catching design. Keep your processor running at optimal temperatures, even under the most demanding workloads, while enjoying customizable A-RGB lighting and the integrated digital temperature display.

**Key selling points:**

* **High-performance air cooling:** 6 direct contact heat pipes and a 120mm A-RGB Pulsar fan ensure efficient and quiet heat dissipation.
* **Digital temperature display:** Monitor your CPU temperature in real-time and adjust the fan speed as needed.
* **Customizable A-RGB lighting:** Create stunning lighting effects that synchronize with your motherboard and other components.
* **Wide compatibility:** Compatible with a wide range of Intel and AMD CPU sockets.
* **Rifle Bearing performance:** Thanks to its Rifle Bearing style bearings, we get the best possible performance, longevity and sound.
* **Easy installation:** The intuitive design and included accessories make installation quick and easy.

**Specifications:**

* **Compatible sockets:** AMD: FM AM3 AM4 AM5 / Intel: LGA 115X/1366/2011/1700/1200/1851
* **Fan:**
  + Model: XYZ PULSAR A-RGB
  + Dimensions: 120 x 120 x 25 mm
  + Bearing: Rifle Bearing
  + Voltage: 10.8 ~ 13.2V
  + Current: 0.28A ±10% MAX
  + Power consumption: 3.36W ±10% MAX
  + Maximum static pressure: 1.78mm-H₂O
  + Lifespan: 50,000 hours at 25°C
  + Number of blades: 9
  + Rotation Speed: 600-1800 ±10% RPM
  + Maximum Air Flow: 78.64 CFM (ft³/min)
  + Max. Noise Level: 36dB(A)
  + Min. Noise Level: 18.5dB(A)
* **Heat pipes:** 6 direct contact copper heat pipes
* **Display:** Integrated digital display with CPU temperature indicator
* **Heatsink dimensions:** 130 x 75 x 158 mm (refer to the manual for exact dimensions)

**Available colours:**   
**White**  
SKU | X-AC-THERPULW6   
  
**Black**  
SKU | X-AC-THERPULB6