**XYZ AQUAPULSE 240 AIO Liquid CPU Cooler,Digital Temperature Display,2x 120mm PWM Pulsar Fans A-RGB**

Master the heat and take your performance to the next level with the **XYZ AQUAPULSE 240** AIO Liquid CPU Cooler. This all-in-one liquid cooling solution combines exceptional performance, sleek aesthetics, and intelligent features to keep your CPU running at optimal temperatures.

**Key Features:**

1. **Digital Temperature Display:** Maintain precise control over your CPU temperature with the digital display integrated into the pump block. Monitor your system's performance in real-time and adjust settings as needed.
2. **Pulsar 120mm PWM A-RGB Fans:** Enjoy quiet and efficient cooling with the two included 120mm Pulsar fans. These PWM fans offer precise speed control and feature customizable ARGB lighting to create a light show in your PC.
3. **Easy Installation:** AQUAPULSE 240 is designed for simple and hassle-free installation, with a universal mounting bracket compatible with a wide range of Intel and AMD sockets.
4. **High-Efficiency Pump:** The high-efficiency pump ensures a constant flow of coolant, maximizing heat dissipation and keeping your CPU running at optimal temperatures even under heavy workloads.
5. **High-Quality Braided Tubing:** The high-quality braided tubing not only offers durability and resistance but also adds an aesthetic touch to your setup.
6. **Wide Compatibility:** AQUAPULSE 240 is compatible with a wide range of Intel and AMD sockets, making it a versatile option for any gaming or high-performance PC.

**General Specifications:**

* **Rated Voltage:** 12V DC
* **Minimum Starting Voltage:** ≤4.0 V
* **Electric Current:** ≤0.30 A
* **Power:** ≤3.6 W
* **Maximum Head:** 1.5M
* **Minimum Flow Rate:** ≥1300 mL/min
* **Speed:** 2500RPM±10%
* **Storage Temperature:** -10°C ~ 70°C
* **Operating Temperature:** -10°C ~ 60°C
* **Minimum estimated lifetime:** 50000 hours under normal working conditions
* **Maximum Noise:** ≤30 db
* **Pump Size:** 67.6 x 82.3 x 55.5 mm (L x W x H)
* **Catheter:** Braided tube L=380 ± 2mm
* **Radiator Dimensions:** 277 x 120 x 27 mm (L x W x H)
* TDP: 250W
* **Socket Support:**
  + Intel: LGA 115X/1366/2011/1700/1200/1851
  + AMD: AM5/AM4

**Technical Specifications - Pulsar 120mm PWM A-RGB Fans**

* **Model:** PULSAR
* **Outside Dimensions:** 120 x 120 x 25 mm
* **Bearing Type:** Rifle Bearing
* **Voltage:**
  + Rated Voltage: DC 12V
  + Operating Voltage: 10.8 ~ 13.2V
  + Starting Voltage: DC 5V MAX
* **Current:**
  + Rated Current: 0.28A ±10% MAX
  + Tag Current: 0.28A ±10% MAX
  + Blocking Current: 0.30A ±10% MAX
* **Power Consumption:** 3.36W ±10% MAX
* **Rotation Speed:** 600-1800 ±10% RPM
* **Maximum Air Flow:** 78.64 CFM (ft³/min)
* **Max. Static Pressure:** 1.78mm-H₂O
* **Max. Noise Level:** 36dB(A)
* **Min. Noise Level:** 18.5dB(A)
* **Minimum Lifetime:** 50,000 hours at 25

**Avaliable Colors:**

**White**

SKU | X-WC-AQUA-240W

EAN | 6978262010379

**Black**

SKU | X-WC-AQUA-240B

EAN | 6978262010355