**XYZ VORTEX PRO A-RGB PWM 3 KIT, Reversed Airflow,Chain System,Fuodinamic Bearing,Premium Performance,2000RPM,ARGB lighting**  
  
Elevate your cooling experience to another dimension with the XYZ Vortex Pro A-RGB fan kit (Reversed Airflow). These high-performance fans deliver exceptional intake capabilities, dazzling ARGB lighting, and seamless wireless connectivity for a pristine gaming setup.

**Key Features:**

* **Maximum Air Intake:** Vortex Pro fans with reversed airflow are designed to efficiently draw cool air into your system, ensuring optimal cooling for your high-performance components, even under the most demanding workloads.
* **Whisper-Quiet Operation:** With a minimum noise level of just 18.5 dB(A), Vortex Pro fans let you enjoy a serene gaming environment without sacrificing performance.
* **Vibrant ARGB Lighting:** Customize your style with the addressable ARGB lighting of the Vortex Pro fans. Synchronize lighting effects with your motherboard and other compatible components to create a mesmerizing visual spectacle.
* **Wireless Daisy-Chaining:** Simplify cable management with the innovative wireless daisy-chain connection of the Vortex Pro fans. Connect up to 3 fans to a single cable, reducing clutter and enhancing the aesthetics of your PC.
* **Durability and Reliability:** Vortex Pro fans are equipped with high-quality FDB bearings and boast a lifespan of up to 60,000 hours, ensuring smooth and long-lasting operation.

**Technical Specifications:**

* **Dimensions:** 120 x 120 x 25 mm
* **Bearing:** FDB (Fluid Dynamic Bearing)
* **Rated Voltage:** DC 12V
* **Operating Voltage:** 10.8 ~ 13.2V
* **Starting Voltage:** DC 5 V MAX
* **Rated Current:** 0.20A ± 20% MAX (Labeled Current: 0.20A)
* **Locked Current:** 0.21A ± 20% MAX
* **Power Consumption:** 2.40W ± 20% MAX
* **Speed:** 600-2000 ± 20% RPM
* **Max. Airflow:** 54.73 CFM (ft³/min)
* **Max. Static Pressure:** 2.05 mm-H₂O
* **Max Noise Level:** 31.4 dB(A)
* **Min. Noise Level:** 18.5 dB(A)
* **Life:** 60,000hrs at 25°C
* **No. of Blades:** 9 Blades
* **No. of Poles:** 4 Poles
* **Airflow:** Reversed (intake)

**Available colors:**

* Black: X-FN-VORPROKIT-BR
* White: X-FN-VORPROKIT-WR